Although **Etcher** makes it extremely easy to flash and prepare SD Cards for the Raspberry Pi, there are other approaches that will allow you to have more fine-grained control around the process. Below are some links to additional documentation for instructions for various Operating Systems.

* Windows
  + <https://www.raspberrypi.org/documentation/installation/installing-images/windows.md>
* Mac
  + <https://www.raspberrypi.org/documentation/installation/installing-images/mac.md>
* Linux
  + <https://www.raspberrypi.org/documentation/installation/installing-images/linux.md>